# Trying port address 0203
# Trying port address 0207
# Trying port address 020b
# Board 1 has serial identifier 6e 00 00 05 d5 00 00 d8 10

# (DEBUG)
(READPORT 0x020b)
(ISOLATE)
(IDENTIFY *)

# Card 1: (serial identifier 6e 00 00 05 d5 00 00 d8 10)
# DFX0000 Serial No 1493 [checksum 6e]
# Version 1.0, Vendor version 1.0
# ANSI string -->Dataflex PC Comms Office<--
#
# Logical device id DFX0001
#     Device support I/O range check register
#
# Edit the entries below to uncomment out the configuration required.
# Note that only the first value of any range is given, this may be changed if required
# Don't forget to uncomment the activate (ACT Y) when happy

(CONFIGURE DFX0000/1493 (LD 0

# Multiple choice time, choose one only !

#     Start dependent functions: priority preferred
#       Fixed IO base address 0x02f8
#             Number of IO addresses required: 8
# (IO 0 (BASE 0x02f8))
#       IRQ 3.
#             High true, edge sensitive interrupt (by default)
# (INT 0 (IRQ 3 (MODE +E)))

#       Start dependent functions: priority acceptable
#       Fixed IO base address 0x02f8
#             Number of IO addresses required: 8
# (IO 0 (BASE 0x02f8))
#       IRQ 3, 4, 5 or 7.
#             High true, edge sensitive interrupt (by default)
# (INT 0 (IRQ 3 (MODE +E)))

#       Start dependent functions: priority acceptable
#       Fixed IO base address 0x02f8
#             Number of IO addresses required: 8
# (IO 0 (BASE 0x02f8))
#       IRQ 3, 4, 5, 7, 9, 10, 11 or 12.
#             High true, edge sensitive interrupt (by default)
# (INT 0 (IRQ 3 (MODE +E)))

#       Start dependent functions: priority acceptable
#       Fixed IO base address 0x03e8
#             Number of IO addresses required: 8
# (IO 0 (BASE 0x03e8))
#       IRQ 3, 4, 5 or 7.
#             High true, edge sensitive interrupt (by default)
# (INT 0 (IRQ 3 (MODE +E)))

#       Start dependent functions: priority acceptable
#       Fixed IO base address 0x03e8
#             Number of IO addresses required: 8
# (IO 0 (BASE 0x03e8))
#       IRQ 3, 4, 5, 7, 9, 10, 11 or 12.
#             High true, edge sensitive interrupt (by default)
# (INT 0 (IRQ 3 (MODE +E)))

#       Start dependent functions: priority acceptable
#       Fixed IO base address 0x02e8
#             Number of IO addresses required: 8
# (IO 0 (BASE 0x02e8))
#       IRQ 3, 4, 5 or 7.
#             High true, edge sensitive interrupt (by default)
# (INT 0 (IRQ 3 (MODE +E)))

#       Start dependent functions: priority acceptable
#       Fixed IO base address 0x02e8
#             Number of IO addresses required: 8
# (IO 0 (BASE 0x02e8))
#       IRQ 3, 4, 5, 7, 9, 10, 11 or 12.
#             High true, edge sensitive interrupt (by default)
# (INT 0 (IRQ 3 (MODE +E)))

#       Start dependent functions: priority acceptable
#       Fixed IO base address 0x03f8
#             Number of IO addresses required: 8
# (IO 0 (BASE 0x03f8))
#       IRQ 4.
#             High true, edge sensitive interrupt (by default)
# (INT 0 (IRQ 4 (MODE +E)))

#       Start dependent functions: priority acceptable
#       Fixed IO base address 0x03f8
#             Number of IO addresses required: 8
# (IO 0 (BASE 0x03f8))
#       IRQ 3, 4, 5 or 7.
#             High true, edge sensitive interrupt (by default)
# (INT 0 (IRQ 3 (MODE +E)))

#       Start dependent functions: priority acceptable
#       Fixed IO base address 0x03f8
#             Number of IO addresses required: 8
# (IO 0 (BASE 0x03f8))
#       IRQ 3, 4, 5, 7, 9, 10, 11 or 12.
#             High true, edge sensitive interrupt (by default)
# (INT 0 (IRQ 3 (MODE +E)))
#       ANSI string -->Modem and Fax<--

#     End dependent functions
# (ACT Y)
))
#
# Logical device id DFX0002
#
# Edit the entries below to uncomment out the configuration required.
# Note that only the first value of any range is given, this may be changed if required
# Don't forget to uncomment the activate (ACT Y) when happy

(CONFIGURE DFX0000/1493 (LD 1

# Multiple choice time, choose one only !

#     Start dependent functions: priority preferred
#       First DMA channel 3.
#             8 bit DMA only
#             Logical device is not a bus master
#             DMA may execute in count by byte mode
#             DMA may not execute in count by word mode
#             DMA channel speed in compatible mode
# (DMA 0 (CHANNEL 3))

#       Start dependent functions: priority acceptable
#       First DMA channel 1.
#             8 bit DMA only
#             Logical device is not a bus master
#             DMA may execute in count by byte mode
#             DMA may not execute in count by word mode
#             DMA channel speed in compatible mode
# (DMA 0 (CHANNEL 1))

#       Start dependent functions: priority acceptable
#       *** ERROR *** No DMA channel specified!
#             8 bit DMA only
#             Logical device is not a bus master
#             DMA may execute in count by byte mode
#             DMA may not execute in count by word mode
#             DMA channel speed in compatible mode
# (DMA 0 (CHANNEL 4))
#       ANSI string -->Voice<--

#     End dependent functions
(ACT Y)))
# End tag... Checksum 0x00 (OK)

